
                            StagCom 95 Windows Application
				   17 September 1998
				  Revision 5.60.95



Programmer Support
------------------

	This version of StagCom Supports the following Programmers:
		ECLIPSE
		ORBIT32
		ORBTI48
                P301
		P800
                P801
		P803  ( minimum flash version required = 3.0 )
		SOLAR
		ZL30B

Notes
-----

	ZL30B Support
	-------------
	
	If the programmer detects that the wrong module is fitted for the
	    currently selected device, then 'Security Fuse Fail.' is displayed,
	    This should be 'Wrong Module Fitted.'.

	If the programmer detects that the wrong device is inserted for the
	    currently selected device, then 'Illegal Bit Pattern.' is displayed.
	    This should be 'Wrong Device Inserted.'.

        SERIALISATION
	-------------

        The 'UNIQUE NUMBER IN ALL SOCKETS' and 'ONE NUMBER IN ONE SOCKET'
        options (available only on multi-socketed programers) will only
        operate correctly if the bitmode set is the same as the width of
        the currently selected device.


Interfacing the Programmer
--------------------------

	For correct serial port operation, the interface connections between 
	PC 25 pin - Programmer 25 pin connectors should be:


 	         Eclipse / Solar               PC

			 PIN                   PIN
		 (SCREEN) 1 ------------------- 1  (SCREEN)
		 (TXD)    2 ------------------- 3  (RXD)
		 (RXD)    3 ------------------- 2  (TXD)
		 (RTS)    4 ------------------- 8  (DCD)
		 (CTS)    5 ------------------- 20 (DTR)
		 (DSR)    6 ------------------- 20 (DTR)
		 (SG)     7 ------------------- 7  (SG)
		 (DCD)    8 ------------------- 4  (RTS)
		 (DTR)    20 ------------------ 5  (CTS)
		 (DTR)    20 ------------------ 6  (DSR)        



	For correct serial port operation, the interface connections between 
	PC 9 pin - Programmer 25 pin connectors should be:

      	         Eclipse / Solar               PC

			 PIN                   PIN
		 (SCREEN) 1 ------------------- 
		 (TXD)    2 ------------------- 2  (RXD)
		 (RXD)    3 ------------------- 3  (TXD)
		 (RTS)    4 ------------------- 1  (DCD)
		 (CTS)    5 ------------------- 4  (DTR)
		 (DSR)    6 ------------------- 4  (DTR)
		 (SG)     7 ------------------- 5  (SG)
		 (DCD)    8 ------------------- 7  (RTS)
		 (DTR)    20 ------------------ 8  (CTS)
		 (DTR)    20 ------------------ 6  (DSR)        
	
	

	For correct serial port operation, the interface connections between 
	PC 25 pin - Programmer 9 pin connectors should be:


	         ORBIT 32/48                       PC

			 PIN                   PIN
 			    ------------------- 1  (SCREEN)
		 (TXD)    3 ------------------- 3  (RXD)
		 (RXD)    2 ------------------- 2  (TXD)
		 (RTS)    7 ------------------- 8  (DCD)
		 (CTS)    8 ------------------- 20 (DTR)
		 (DSR)    6 ------------------- 20 (DTR)
		 (SG)     5 ------------------- 7  (SG)
		 (DCD)    1 ------------------- 4  (RTS)
		 (DTR)    4 ------------------- 5  (CTS)
		 (DTR)    4 ------------------- 6  (DSR)        



	For correct serial port operation, the interface connections between 
	PC 9 pin - Programmer 9 pin connectors should be:


		 ORBIT 32/48                      PC

			 PIN                   PIN
		 (TXD)    3 ------------------- 2  (RXD)
		 (RXD)    2 ------------------- 3  (TXD)
		 (RTS)    7 ------------------- 1  (DCD)
		 (CTS)    8 ------------------- 4  (DTR)
		 (DSR)    6 ------------------- 4  (DTR)
		 (SG)     5 ------------------- 5  (SG)
		 (DCD)    1 ------------------- 7  (RTS)
		 (DTR)    4 ------------------- 8  (CTS)
		 (DTR)    4 ------------------- 6  (DSR)        
