Special Instructions for EMP Software under Windows NT
=============================================

The driver for Windows NT requires that the EMP software be run in  !! full screen !!!.  

It will not be able to communicate with the Device Programmer in a window.

A MSDOS window can be switched to full screen by using the <ALT><Enter> key sequence.
This toggles from the graphical based window to the text based full screen mode.

A Short-Cut or Icon can be made to automatically
run the EMP software full screen by using the PIF 
editor(WinNT 3.51 or earlier), or by right clicking on 
the Short-Cut(WinNT 4.0 or later), and changing the 
properties to full screen.  It is also recommended to
not allow the screen saver, always suspend in 
background mode, and set idle sensitivity to low.
